Download the firmware to control board using Xloader

1. Open Xloader software to open GRBL0.9.hex (or other name) file

2. Select Nano board

3, select the serial number on the serial number of the computer itself (how to check the serial number, please look at Baidu).

4. Click upload;

5. After a few seconds the display xxxx byte uploaded it.
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